HELP – from any point in menus, Spacebar + h

Visual Display Mode: allows teacher to see what is being done currently within a Braillenote document. It also gives a visual representation of the Braille display.

Connections: switch on Braillenote before putting cable in.

Screen (laptop, PC or other e.g. small portable screen) needs to have had programme loaded from Humanware disc or website.  When loading, programme will ask “which com port?” In older machines with serial port, it will be com 1. In newer machines with no serial port, you need to by a “usb to serial connection” and the programme will assign a com number to it.

Connect Braillenote to laptop or PC or other: (remember might be via two linked cables if no serial port on laptop or pc)

Cables: “compact flash vga cable”, or, on pc, “usb to serial port”

To get it going: space + o for options



       v for visual display

it will announce current mode – either turn on using s for serial or use f for off (if you want to use serial port for something else, like the embosser)

New Keyview programme also available. Download possible depending on version of software.

From laptop or PC screen, you can copy and paste into a word document. This operates like a camera shot, and only captures what can be seen at any time, but you can move down the Braillenote document and repeat.

Visual display programme can also be used via the Bluetooth connection.

With Whiteboard/Smartboard? Most take vga cables. Would this need to done via the class teacher’s  computer?

Voice options: o + spacebar (options)

Then, r

scroll through to voice options

e for eloquence
press enter

default male voice

Font: check document set up

Spacebar + the   for format menu

Can change font (1 or 2 choices), line spacing (1.0, 1.5, 2.0), print setting margins, but NOT size (always N12).

 ‘append’ allows copying of several items to clipboard without losing previous, as you do in ‘copy’

